Following our discussion, we have agreed to proceed with using two rows of bolts for the attachment of the plate to the T profile, as indicated in the sections. This decision is due to the constraint posed by the T profile's flange running along the middle, preventing a row of bolts down the center.

Please consider this email as confirmation of our choice to utilize two rows of bolts for the installation.

Thank you, and please let me know if you have any further questions.